Positions quoted in this Preliminary Notice reproduced below are referred to WGS84 or a compatible datum and may be plotted directly on this ENC. 		
Some or all of the information contained in this Notice to Mariners may have been included on the ENCs affected.		
		
3822(P)/25 CHINA —  East Coast — Overhead cable. Vertical clearance.		
Source: Globe Polaris		
		
	1.	It has been reported that the overhead power cable, with a charted vertical clearance of 36m, in position: 29° 43' .91N. , 122° 13' .03E. , has been removed.
		
	2.	Charts will be updated when full details are available.
		
		(CGCS 2000 DATUM)