Positions quoted in the Temporary Notice reproduced below are referred to WGS84 or a compatible datum and may be plotted directly on this ENC.
Some or all of the information contained in this Notice to Mariners may have been included in the ENCs affected.

706(T)/21 UNITED STATES OF AMERICA — West Coast — — Disused submarine cable. Foul. 
Source: US Coast Guard District 11 LNM 2/18650/21

	1. A disused submarine power cable has been reported to foul anchors in Anchorage 8 in the vicinity of position 37° 47' .58N. , 122° 21' .48W. 

	2. Mariners are advised to navigate with caution in the area.

	3. For further information contact USCG Sector San Francisco Waterways Management at SFWaterways@uscg.mil

	   (NAD83 DATUM)