Positions quoted in this Preliminary Notice reproduced below are referred to WGS84 or a compatible datum and may be plotted directly on this ENC.	
Some or all of the information contained in this Notice to Mariners may have been included on the ENCs affected.		
		
3465(P)/24 CHINA —  East Coast — Overhead cable. Safe vertical clearance.		
Source: mv Stena Superior and mv Tenryu		
		
	1.	*It has been reported that the overhead power cable, with a charted vertical clearance of 36m, in position 29° 43' .89N. , 122° 13' .12E. , now has a vertical clearance of 72·5m.
		
	2.	It has been reported that the vertical clearance of the overhead power cable, in position 29° 43' .82N. , 122° 13' .52E. , has been reduced to 70m.
		
	3.	Mariners are advised to navigate with caution in the area and consult the local port authorities for the latest information.
		
	4.	Charts will be updated when full details are available.
		
	5.	* Former Notice 5350(P)/21 is cancelled.
		
		(CGCS 2000 DATUM)