SBM 1 BERTHING RESTRICTIONS
1. Vessels up to length 244m and draft up to 12m should use SBM 1.
2. Vessel should arrive to pilot board station latest by about 1500 hrs in order not to miss daylight pilotage/ berthing.
3. Unberthing could be done night time and subject to pilot decision. 
4. 12 inch loading house will be connected to the port side manifold using the vessel's crane which must have a minimun SWL 15 tons.

