RØDSAND 2 WIND FARM
Air obstruction lights (R.Lts and Lts) on all 90 windmotors. 
Recording stations marked by yellow buoys or yellow light buoys
(Fl(5)Y.20s) are established in the wind farm.
Anchoring and any use of gear towed on the bottom are prohibited within 
the submarine cable area which is established with a protection zone 
extending 200 metres around the wind farm and the transformer platform.