BERTHING RESTRICTIONS
1. Vessels up to length 274m and draft up to 16.3m should use SBM 2.
2. Vessel should arrive to pilot board station latest by about 1400 hrs in order not to miss daylight pilotage/ berthing.
3. Unberthing could be done night time and subject to pilot decision.  
4. 16 inch loading house will be connected to the port side manifold using the vessel's crane which must have a minimun SWL 15 tons.
