INTRACOASTAL WATERWAY PROJECT DEPTHS
The project depth is 2.7 meters/9 feet from Caloosahatchee River, FL. to Anclote River, FL. The controlling depths are published periodically in the U.S. Coast Guard Local Notice to Mariners.