Direction of leading line's axis making by synchronize scanning by laser lights of lighting beacon 4670.1 and 4670.2. During passage of vessel to leading line laser lights observed like simultaneous flashes. If vessel shifted from midchannel laser lights observed at different time like two consistent flashes