Sailing directions
Vessels underway to the harbour should, starting from the KUZ light buoy, steer the course 335°. After passing the Nr 2 buoy to the portside then smoothly align themselves with the KUZNICA leading line (Krk 339°).
Navigating in the channel, the vessels should exercise caution and watch the shallow areas existing on either side of the channel.