SUBMARINE CABLES

Submarine power cables may conduct high voltages; contact with these poses an extreme danger and mariners may risk prosecution if damage is caused. Mariners should not anchor within 2 miles of the power cables laid in this area.