DEPTHS

Depths in the maintained area are 
generally maintained, but silting is liable 
to occur around the area of the second pair 
of lateral buoys and in the southeast part 
of the maintained area in Basin I.

For the latest information, consult the 
Harbour Master's Office.
