Sailing Directions: From the SWB buoy, mariners are advised to steer a course 260°, exercising extreme caution due to shaoling, with depths reduced to 1.4 meters. After pasing the eastern guide pier of the Vistula Cut to port, the course should be altered to 207°.