PARALLEL SHIPPING SAFETY FAIRWAYS
These are parallel shipping safety fairways and not a traffic separation scheme. However, in the interest of vessel traffic safety use of the northeast lane for inbound (298° true) traffic  and the southwest lane for outbound (118° true) traffic is recommended.