OUTER ANCHORAGE
Vessels with an overall length of between 200m and 350m are required to anchor at anchor berths 
designated A or B. Vessels under 200m in overall length are to anchor at anchor berths 
designated 1, 2, 3, 4, 5 or 6. For further details, see Admiralty Sailing Directions.For vessels 
with a draught exceeding 10.0m. Mariners are to contact Dammam Port Control on Channel 16 for 
further instructions before entering the anchorage area.