ENC LT562520


DEPTHS AND HEIGHTS (EVRS 07)

Recalculating the depths and heights from the Mean Sea Level of the Baltic Height System (BHS77) into the European Vertical Reference System (EVRS07) and Lithuanian Height System (LHS07), the depth values  on the chart need to be reduced by 0.13 meters (-13 cm) and the heights must be increased by 0.13 meters (+13 cm).


VESSEL TRAFFIC SERVICE

Radio contact by VHF - 16, 9, call sign Klaipeda radio-5;
VHF channels 16, 71, call sign Terminal control.


CAUTION - BUTINGE OIL TERMINAL

Shipping, maneuvering, fishing or other activity in Butinge oil terminal area, tankers fairway and tankers anchorage area are prohibited, except ships passing to the terminal for load or unload cargo and terminal service ships.


HISTORIC WRECKS

The sites of historic wreck are protected from unauthorised exploration and interference. Zones 500 m in radius have been established around such wrecks.


ENVIRONMENTALLY SENSITIVE SEA AREA (ESSA), MARINE RESERVE (MR)

Certain restrictions apply within the area indicated on this chart.To avoid the risk of pollution and damage to the environment in this area. For detailed information refer to publication Shipping Regulations.


FISHING  NETS

Uncharted fishing nets can be laid in Lithuanian coastal areas inside the 20 m depth contour.


LITHUANIA - LATVIA MARITIME BORDER

Agreement regarding sea boundary determination is not ratified.