SAFETY BROADCASTS

All vessels of LOA 20 metres and greater entering or leaving Oban Bay by the northern entrance, are requested to broadcast a warning message on VHF Channel 16, followed by a more detailed message on VHF Channel 12. For details, see Admiralty List of Radio Signals and the Code of Practice for Oban Bay.


