Midchannel direction  92.1° axis is assigned by synchronized scanning of laser beams of Gates 19 left  and Gates 19 right light beacons.
When vessel is moving along Midchannel axis the laser beams are seen as two simultaneous flashes. 
When vessel shifts from Midchannel axis the laser beams are seen at different times as two sequential flashes