NOAA ENCŪ

NATIONAL OCEANIC AND ATMOSPHERIC ADMINISTRATION

US5CA60M - GULF OF SANTA CATALINA - DANA POINT HARBOR, CA


INDEX:

NOTE A
AUTHORITIES
AIDS TO NAVIGATION
SUPPLEMENTAL INFORMATION
WARNING - PRUDENT MARINER
POLLUTION REPORTS
RADAR REFLECTORS
ADMINISTRATION AREA
CAUTION - TEMPORARY CHANGES
CAUTION - LIMITATIONS
CAUTION - SUBMARINE PIPELINES AND CABLES
CAUTION - USACE HYDROGRAPHIC SURVEYS
NOAA WEATHER RADIO BROADCASTS
MINERAL DEVELOPMENT STRUCTURES
CAUTION - QUALITY OF BATHYMETRIC DATA
WATER LEVELS, CURRENTS, AND TIDES
COMMENTS REQUESTED
ADDITIONAL INFORMATION


NOTES:

NOTE A 
Navigation regulations are published in Chapter 2, U.S. Coast Pilot 7. Additions or revisions to Chapter 2 are published in the Notice to Mariners. Information concerning the regulations may be obtained at the Office of the Commander, 11th Coast Guard District in Alameda, California or at the Office of the District Engineer, Corps of Engineers in Los Angeles, California.
Refer to charted regulation section numbers. 


AUTHORITIES 
Hydrography and topography by the National Ocean Service, Coast Survey, with additional data from the Corps of Engineers, Geological Survey, U.S. Coast Guard and Department of the Navy.


AIDS TO NAVIGATION 
Consult U.S. Coast Guard Light List for supplemental information concerning aids to navigation.


SUPPLEMENTAL INFORMATION 
Consult U.S. Coast Pilot 7 for important supplemental information.


WARNING - PRUDENT MARINER 
The prudent mariner will not rely solely on any single aid to navigation, particularly on floating aids. See U.S. Coast Guard Light List and U.S. Coast Pilot for details.


POLLUTION REPORTS 
Report all spills of oil and hazardous substances to the National Response Center via 1-800-424-8802 (toll free), or to the nearest U.S. Coast Guard facility if telephone communication is impossible (33 CFR 153).


RADAR REFLECTORS 
Radar reflectors have been placed on many floating aids to navigation. Individual radar reflector identification on these aids has been omitted from this chart.


ADMINISTRATION AREA
The entire extent of this ENC cell falls within the limits of an Administration Area. This area covers land, internal waters, and territorial sea.  The territorial sea is a maritime zone which the United States exercises sovereignty extending to the airspace as well as to its bed and subsoil.  For more information, please refer to the Coast Pilot.


CAUTION - TEMPORARY CHANGES
Temporary changes or defects in aids to navigation are not indicated. See Local Notice to Mariners.


CAUTION - LIMITATIONS
Limitations on the use of radio signals as aids to marine navigation can be found in the U.S. Coast Guard Light Lists and National Geospatial-Intelligence Agency Publication 117. Radio direction-finder bearings to commercial broadcasting stations are subject to error and should be used with caution.


CAUTION - SUBMARINE PIPELINES AND CABLES
Additional uncharted submarine pipelines and submarine cables may exist within the area of this chart. Not all submarine pipelines and submarine cables are required to be buried, and those that were originally buried may have become exposed. Mariners should use extreme caution when operating vessels in depths of water comparable to their draft in areas where pipelines and cables may exist, and when anchoring, dragging, or trawling. Covered wells may be marked by lighted or unlighted buoys.


CAUTION - USACE HYDROGRAPHIC SURVEYS
USACE conducts hydrographic surveys to monitor navigation conditions. These surveys are not intended to detect underwater features. Uncharted features hazardous to surface navigation may exist in federal channels, as might shoaling, particularly along the edges of channels. For more information visit https://navigation.usace.army.mil/Survey/Hydro/ .


NOAA WEATHER RADIO BROADCASTS
The NOAA Weather Radio stations listed below provide continuous weather broadcasts. The reception range is typically 37 to 74 kilometers / 20 to 40 nautical miles from the antenna site, but can be as much as 185 kilometers / 100 nautical miles for stations at high elevations.

Los Angeles, CA	  KWO-37	162.550 MHz
Santa Ana, CA	  WWG-21	162.450 MHz
Santa Diego, CA	  KEC-62	162.400 MHz


MINERAL DEVELOPMENT STRUCTURES
Obstruction lights and sound (fog) signals are required for fixed mineral development structures shown subject to approval by the District Commander, U.S. Coast Guard (33 CFR 67).


CAUTION - QUALITY OF BATHYMETRIC DATA
The areas represented by the object M_QUAL are approximate due to generalizing for clarity. Caution is advised, particularly for nearshore navigation or voyage planning. M_QUAL (Quality of data) represents areas of uniform quality of bathymetric data. The CATZOC (Category of zone of confidence in data) attribute of M_QUAL provides an assessment of the overall zone of confidence.


WATER LEVELS, CURRENTS, AND TIDES
Real-time water levels, tide predictions, and tidal current predictions are available on the internet from NOAA's Center for Operational Oceanographic Products and Services (CO-OPS) at https://tidesandcurrents.noaa.gov/water_level_info.html and https://tidesandcurrents.noaa.gov/currents_info.html.


COMMENTS REQUESTED
NOAA encourages users to submit inquiries, discrepancies, or comments about this chart via NOAA's ASSIST tool at https://www.nauticalcharts.noaa.gov/customer-service/assist/.


ADDITIONAL INFORMATION
Additional information can be obtained at www.nauticalcharts.noaa.gov.


END OF FILE
