Designated Route in the North of Osaka Wan
 1. Vessels which are of 500G/T and upwards and will navigate by crossing Line B after crossing
    Line A should navigate in the area to the north of Line C.
 2. Vessels which are of 500G/T and upwards and will navigate by crossing Line A after crossing
    Line B should navigate in the area to the south of Line C.
 3. For detailed information on the designation of tracks, refer to the Japan Coast Guard
    Notification No 92 dated 1st April 2010.
--------
New,20100701,JP,JP,graph,chart0150A
