NOAA ENCŪ

NATIONAL OCEANIC AND ATMOSPHERIC ADMINISTRATION

US5WA1BE - PORT ANGELES, WA


INDEX:

NOTE A
AIDS TO NAVIGATION
POLLUTION REPORTS
CAUTION - USE OF RADIO SIGNALS (LIMITATIONS)
SUPPLEMENTAL INFORMATION
CAUTION - TEMPORARY CHANGES
WARNING - PRUDENT MARINER
ADDITIONAL INFORMATION
AUTHORITIES
ANCHORING STANDARDS OF CARE
CAUTION - QUALITY OF BATHYMETRIC DATA
CAUTION - SUBMARINE PIPELINES AND CABLES
COLREGS, 80.1385
LIGHTERING STANDARDS OF CARE
MANDATORY VESSEL TRAFFIC SERVICES
NOAA WEATHER RADIO BROADCASTS
NOTE D
PUGET SOUND HARBOR SAFETY PLAN
RADAR REFLECTORS
SMALL ARMS SAFETY ZONE
WATER LEVELS, CURRENTS, AND TIDES
COMMENTS REQUESTED


NOTES:

NOTE A
Navigation regulations are published in Chapter 2, U.S. Coast Pilot 10. Additions or revisions to Chapter 2 are published in the Notices to Mariners. Information concerning the regulations may be obtained at the Office of the Commander, 13th Coast Guard District in Seattle, Washington or at the Office of the District Engineer, Corps of Engineers in Seattle, Washington. Refer to charted regulation section numbers.


AIDS TO NAVIGATION
Consult U.S. Coast Guard Light List for supplemental information concerning aids to navigation.


POLLUTION REPORTS
Report all spills of oil and hazardous substances to the National Response Center via 1-800-424-8802 (toll free), or to the nearest U.S. Coast Guard facility if telephone communication is impossible (33 CFR 153).


CAUTION - USE OF RADIO SIGNALS (LIMITATIONS)
Limitations on the use of radio signals as aids to marine navigation can be found in the U.S. Coast Guard Light Lists and National Geospatial-Intelligence Agency Publication 117. Radio direction-finder bearings to commercial broadcasting stations are subject to error and should be used with caution.


SUPPLEMENTAL INFORMATION
Consult U.S. Coast Pilot 10 for important supplemental information.


CAUTION - TEMPORARY CHANGES
Temporary changes or defects in aids to navigation are not indicated. See Local Notice to Mariners.


WARNING - PRUDENT MARINER
The prudent mariner will not rely solely on any single aid to navigation, particularly on floating aids. See U.S. Coast Guard Light List and U.S. Coast Pilot for details.


ADDITIONAL INFORMATION
Additional information can be obtained at WWW.nauticalcharts.noaa.gov.


AUTHORITIES
Hydrography and topography by the National Ocean Service, Coast Survey with additional data from the Corps of Engineers, Geological Survey, and U.S. Coast Guard.


ANCHORING STANDARDS OF CARE
Anchoring Standards of Care have been established for this area through the Harbor Safety Plan. These Standards of Care supplement existing regulations with good marine practices for anchoring, and are separated into different weather categories. If your vessel does not have a copy of the Anchoring Standards of Care, you can download one at https://marexps.com/membership/puget-sound-harbor-safety-committee/ or contact the Marine Exchange of Puget Sound at (206) 443-3830.


CAUTION - QUALITY OF BATHYMETRIC DATA
The areas represented by the object M_QUAL (Quality of data) are approximate due to generalizing for clarity. Caution is advised, particularly for nearshore navigation or voyage planning. M_QUAL represents areas of uniform quality of bathymetric data. The CATZOC (Category of zone of confidence in data) attribute of M_QUAL provides an assessment of the overall zone of confidence.


CAUTION - SUBMARINE PIPELINES AND CABLES
Additional uncharted submarine pipelines and submarine cables may exist within the area of this chart. Not all submarine pipelines and submarine cables are required to be buried, and those that were originally buried may have become exposed. Mariners should use extreme caution when operating vessels in depths of water comparable to their draft in areas where pipelines and cables may exist, and when anchoring, dragging or trawling. Covered wells may be marked by lighted or unlighted buoys.


COLREGS, 80.1385
International Regulations for Preventing Collisions at Sea, 1972. The entire area of this chart falls seaward of the COLREGS Demarcation Line.


LIGHTERING STANDARDS OF CARE
Lightering Standards of Care have been established for this area through the Harbor Safety Plan. These Standards of Care supplement existing regulations with good marine practices for lightering. If your vessel does not have a copy of the Lightering Standards of Care, you can download one at https://marexps.com/membership/puget-sound-harbor-safety-committee/ or contact the Marine Exchange of Puget Sound at (206) 443-3830.


MANDATORY VESSEL TRAFFIC SERVICES
The U.S. Coast Guard operates a mandatory Vessel Traffic Services (VTS) system in the U.S. Waters covered by this chart. Vessel operating procedures and designated radio-telephone frequencies are published in 33 CFR 161, the U.S. Coast Pilot, and/or the VTS User's Manual.


NOAA WEATHER RADIO BROADCASTS
The NOAA Weather Radio stations listed below provide continuous weather broadcasts. The reception range is typically 37 to 74 kilometers / 20 to 40 nautical miles from the antenna site, but can be as much as 185 kilometers / 100 nautical miles for stations at high elevations.

Neah Bay, WA		KIH-36		162.550 MHz
Puget Sound Marine, WA		WWG-24		162.425 MHz


NOTE D
One-way traffic lanes on this chart are RECOMMENDED for use by all vessels traveling between the points involved. They have been designated to aid in the prevention of collisions in the Strait of Juan De Fuca water, but are not intended in any to supersede or alter the applicable Rules of the Road. Separation Zones are intended to separate inbound and outbound traffic and to be free of ship traffic. Separation Zones should not be used except for crossing purposes. When crossing traffic lanes and separation Zones, use extreme caution.

Precautionary Areas have been established where major lanes merge and cross the traffic separation scheme. It is recommended that vessels proceed with caution in these areas. Wherever practical, vessels entering or leaving the system should do so at these precautionary areas. For more information regarding Traffic Separation Scheme procedures and regulations, see 33 CFR 167 and/or Chapter 2 of the U.S. Coast Pilot.


PUGET SOUND HARBOR SAFETY PLAN
The US Coast Guard and the Puget Sound Harbor Safety Committee have developed and adopted a Harbor Safety Plan that formally established a set of Standards of Care for Puget Sound and surrounding waters. These Standards of Care are intended to supplement existing regulations by documenting good marine practices for a variety of operations including tug escorts, pilotage, anchoring, lightering, and provides additional information on required charts, Aids to Navigation and Emergency Response. If your vessel does not already have a copy of the Puget Sound Harbor Safety Plan, visit https://marexps.com/membership/puget-sound-harbor-safety-committee/ or contact the Marine Exchange of Puget Sound at (206) 443-3830.


RADAR REFLECTORS
Radar reflectors have been placed on many floating aids to navigation. Individual radar reflector identification on these aids has been omitted from this chart.


SMALL ARMS SAFETY ZONE
Naval Air Station small arms range operates 7 days a week. Red flashing light and flags are displayed during live fire exercises. Use caution when transiting near the zone.


WATER LEVELS, CURRENTS, AND TIDES
Real-time water levels, tide predictions, and tidal current predictions are available on the internet from NOAA's Center for Operational Oceanographic Products and Services (CO-OPS) at https://tidesandcurrents.noaa.gov/water_level_info.html and https://tidesandcurrents.noaa.gov/currents_info.html.


COMMENTS REQUESTED
NOAA encourages users to submit inquiries, discrepancies, or comments about this chart via NOAA's ASSIST tool at https://www.nauticalcharts.noaa.gov/customer-service/assist/.


END OF FILE
