ENC LT381002 (LITHUANIAN EXCLUSIVE ECONOMIC ZONE. Western PART (90 000))


DEPTHS AND HEIGHTS IN NEW CHART DATUM BSCD2000 (LAS07)!

Recalculating the depths and heights from the Baltic Sea Chart Datum 2000 (BSCD2000, national realization LAS07) into the Mean Sea Level of the Baltic Height System (BHS77), the charted depth values must be increased by 0.13 metres (+13 cm), while the height values must be reduced by 0.13 metres (-13 cm).


VESSEL TRAFFIC SERVICE

Radio contact by VHF channel 9, call sign Klaipeda radio-5;
VHF channel 71, call sign Terminal control;
VHF channel 10, call sign Klaipeda radio-32.

WRECKS - GENERALIZATION

Not all wrecks and obstructions are not charted between the shoreline and 20 m depth contour. Details see charts at larger scales.


FORMER MINED AREA

Former Mined Areas are open for navigation. It is not advised to anchor, trawl, dredge or conduct 
other operations near the seabed, as danger of possible mines and other explosives exists in these 
areas.

MILITARY PRACTICE AREA

Due to the danger to safe navigation, shipping may be temporarily restricted during military 
exercises in the military practice areas. Information on military exercises is disseminated via 
NAVTEX and provided on the Administration's website.


EXPLOSIVES DUMPING GROUND

Anchoring, trawling, carrying out underwater explosions and other underwater activities are 
prohibited in this area. 

SPOIL GROUND

Depths in Spoil Ground Areas may be less than charted.


HISTORIC WRECKS

The sites of historic wreck are protected from unauthorised exploration and interference. Zones of 150 to 500 m in radius have been established around such wrecks.

SUBMARINE CABLE

Anchoring, fishing, and any underwater works are prohibited within a safety zone extending 100 
metres on both sides of the submarine cable. 


LITHUANIA - LATVIA MARITIME BORDER

Agreement regarding sea boundary determination is not ratified.