TUG BOAT ESCORT TO/FROM BROFJORDEN
All crude oil tankers and loaded product tankers > 20 000 DW
are required to be escorted by tugs from the
waters 3 M southwest of buoy Brofjorden Approach.
It is not recommended to meet or overtake an escorted 
crude oil tanker in the area between buoys Brofjorden 
Nr 1 and Nr 2 and a line between buoys Hästebåden
and Kornögrundet. When other ships are escorted in
this part of the fairway, it is recommended that meeting
and overtaking is done with great caution.
