MAGNETIC COMPASS DEFLECTIONS
Magnetic compass deflections of up to 70° can
occur near the high-voltage direct-current cable.
Switch off your magnetic compass autopilot before
you sail across the cable. Whenever possible, do
so quickly and at a right angle. See "Seehandbuch".