this area is intended for the protection of submarine pipelines. three loading berths are located within this area.
within this area:
-anchoring is prohibited
-only tankers assigned to a designated loading berth are permitted to operate within this area.as well as service vessels.
-the loading berths located in this area are accessible only to vessels with a maximum deadweight of 13,000 tonnes, fully laden, and with a minimum overall length of 165 metres.