OBAN BAY CODE OF PRACTICE – NARROW CHANNELS

Vessels navigating in Oban Bay and approaches should be aware of the existence of a voluntary code for safe navigation within the area, which may be found at www.obanharbour.scot. Vessels navigating in this area should be considered to be in Narrow Channels within the meaning of Rule 9 of the International Regulations for Preventing Collisions at Sea (1972). The speed limit in Oban Harbour is 6 knots.


