ANCHORAGE AREAS.                      
Anchorage area No 1 is reserved for vessels with a draught of 6 m and over.
Vessels with lesser draught than 6 m are referred to Anchorage area No 2 
and it is recommended that this anchorage area is not used with a larger draught.
Anchorage area No 3 is reserved for vessels bound for Koebenhavns Havn.
Attention is drawn to the fact that vessels are not, except when
urgently necessary, allowed to anchor on leading lines or in such
a manner that may interfere or hinder the safe passage of other
vessels. Offences shall be punishable by fine.
