Chart Number: 3911
S-57 ENC Number: CA570450

CABLES The symbols for submarine and overhead cables do not differentiate between cables conducting electric power, often at high voltages, and other types of utility cables. Mariners are advised to exercise caution when passing under all overhead cables and to avoid anchoring or conducting seabed operations in the vicinity of submarine cables. The clearance of an overhead cable may differ from its charted value due to changes in atmospheric conditions, water levels and other factors. For additional information, consult Notice No. 16 in the Notices to Mariners, Annual Edition and the appropriate volume of CHS Sailing Directions.

Current velocities represent normal maximum rates at springs

See Canadian Tide and Current Tables Vol. 7 for current information.

See Notices to Mariners for subsequent corrections on this chart and Notices to Shipping in force for hazards or changes essential for the safety of navigation.

© Fisheries and Oceans Canada 2015 / Pêches et Océans Canada 2015. Published by the Canadian Hydrographic Service / Publié par le Service hydrographique du Canada. A licence is required from the Canadian Hydrographic Service (www.charts.gc.ca) to reproduce or distribute this work. La reproduction et la distribution de ce produit sont sujettes à l’obtention d’un permis octroyé par le Service hydrographique du Canada (www.charts.gc.ca).