S-57 ENC Number: CA471181

CABLES The symbols for submarine and overhead cables do not differentiate between cables conducting electric power, often at high voltages, and other types of utility cables. Mariners are advised to exercise caution when passing under all overhead cables and to avoid anchoring or conducting seabed operations in the vicinity of submarine cables. The clearance of an overhead cable may differ from its charted value due to changes in atmospheric conditions, water levels and other factors. For additional information, consult Notice No. 16 in the Notices to Mariners, Annual Edition and the appropriate volume of CHS Sailing Directions.

Current velocities represent normal maximum rates at springs. 

See Canadian Tide and Current Tables Vol. 6 for current information.

MOORING BUOYS Private mooring buoys exist in this area, most established for recreational use. Due to the number of buoys and the frequency of change, individual buoys are not charted. Many do not comply with Canadian Coast Guard standards and are difficult to see.

VESSEL TRAFFIC SERVICES Traffic Services calling-in point with number; arrow indicates direction of vessel movement. For additional information concerning these services, see Radio Aids to Marine Navigation, Part 3.

See Notices to Mariners for subsequent corrections on this chart and Notices to Shipping in force for hazards or changes essential for the safety of navigation.

© His Majesty the King in Right of Canada, as represented by the Minister of the Department of Fisheries and Oceans, 2023. Published by the Canadian Hydrographic Service.  A licence is required from the Canadian Hydrographic Service (www.charts.gc.ca) to reproduce or distribute this work.
