
DEPTHS AND HEIGHTS (EVRS 07)

Recalculating the depths and heights from the Mean Sea Level of the Baltic Height System (BHS77) into the European Vertical Reference System (EVRS07) and Lithuanian Height System (LHS07). Depths shown on nautical charts will be reduced by 13 cm (-13 cm), depending on particular area. Heights will be increased by 13 cm (+13 cm).


VESSEL TRAFFIC SERVICE

Radio contact by VHF channel 9, call sign Klaipeda radio-5;
VHF channel 71, call sign Terminal control;
VHF channel 10, call sign Klaipeda radio-32.


WRECKS - GENERALIZATION

Not all wrecks and obstructions are not charted between the shoreline and 20 m depth contour.Details see charts at larger scales.


ENVIRONMENTALLY SENSITIVE SEA AREA (ESSA), MARINE RESERVE (MR)

To avoid the risk of pollution and damage to the environment in these areas, certain restrictions apply within the area indicated on this chart. For further details see the publication "Shipping Regulations".


FORMER MINED AREA, OPENED FOR NAVIGATION

Former Mined Areas, opened for navigation. Ships are not advised to anchor, trawl, dredge, proceed with a stack anchor or conduct other operations near the seabed, as danger of mines and other explosives exists in this area.


MILITARY PRACTICE AREA

Area is dangerous to navigation for the period of dangerous operations conduct. The time of dangerous operations conduct and promulgated via NAVTEX 5 days in advance before the commencement of these operations.


FORMER MILITARY PRACTICE AREA (Area No 102)

Vessels are not advised to anchor, trawl, proceed with a slack anchor and carry out other operations near the seabed, as danger of mines and other explosives exists in this area.


FISHING  GROUND

Caution is advised for transiting ships due to fishing gears that could obstruct shipping safety. Uncharted fishing nets may be laid in Lithuanian coastal areas inside the 20 m depth contour.


BUTINGE OIL TERMINAL

Only authorised vessels may enter the tanker anchorage,tanker transit area and the terminal are associated with Butiinge Oil Terminal.


EXPLOSIVES DUMPING GROUND

Anchoring, bottom fishing, underwater works and underwater explosions are prohibited in these areas.


SPOIL GROUND

Depths in Spoil Ground Areas may be less than charted.


HISTORIC WRECKS

The sites of historic wreck are protected from unauthorised exploration and interference. Zones of 150 to 500 m in radius have been established around such wrecks.


SUBMARINE CABLE

Anchoring, fishing and any underwater works are prohibited within a safety zone extending 100 m on both sides of the submarine cable.


LITHUANIA - LATVIA MARITIME BORDER

Agreement regarding sea boundary determination is not ratified.








