INWARDS REPORTING

All vessels bound inwards to Fremantle are to
report to Port of Fremantle when crossing the
reporting line (VHF 12).
Vessels are required to report their confirmation
of pilotage requirement for either the Outer or 
Inner Pilot Boarding Ground.
Vessels proceeding to the Inner Pilot Boarding 
Ground or to anchorage in Gage Roads (draught 
less than 11m) are required to indicate their 
intended route.
Port of Fremantle is able to provide VTS
information relating to shipping movements.
