FRENCH REGULATIONS

Vessels exceeding 1600 GT laden with hydrocarbons or other dangerous cargoes must keep at least 7 miles off the French coast, except when entering certain ports. For further details, see Admiralty Sailing Directions.