LADEN TANKERS


Laden tankers over 10,000 gt using the Traffic Separation Scheme Off Land’s End, between Seven 
Stones and Longships ,should keep at least 3 miles to seaward of Wolf Rock and should not use the 
scheme in restricted visibility or other adverse weather. For reporting procedures, see Admiralty list 
of Radio Signals.

