NYSTED WIND FARM
Due to the risk of collapsing of windmotors navigation within a distance of 200 m from the wind farm is not recommended until further notice.
Air obstruction lights (R.Lts) on all 72 windmotors. Through the wind farm, from the SW corner to the NE corner, 16 windmotors in pair are painted on circular, red respectively green daymarks according to the lateral marks system. 
Recording stations marked by yellow buoys or yellow light buoys (Fl(5)Y.20s) are established in the wind farm.
Anchoring and any use of gear towed on the bottom are prohibited within the submarine cable area which is established with a protection zone extending 200 metres around the wind farm and the transformer platform.