CAUTION - CHANGING DEPTHS

The banks off Great Yarmouth and Lowestoft and depths in the approaches to these ports are continually changing. For example, a survey in 2011 recorded a 0.3 metre drying height where the charted depths were 12 metres. Mariners are strongly advised to use the buoyed channels and to take a pilot before entering port.