SCIENTIFIC MOORINGS Acoustic sensors, consisting of a concrete anchor and tethered instrument package floating above the anchor, are positioned approximately 1 km apart along the line. Instruments in water less than 150m deep are within 5m of the seabed. Instruments in water more than 150m deep are approximately 150m below the surface.