WARNING
The navigator should not rely entirely on floating navaids, as they could be out of position due to various factors.

NOTES
1.- Sailors must observe the current regulations, issued by the competent authority, for navigation in the aquatic spaces covered by this charter.
2.- Chart limits to the next larger scale appear in magenta. Users should consult the Catalog of Nautical Charts on the INOCAR website, which may contain more recent information.
3.- It is forbidden for a vessel to overtake another in the following section of the access channel (Estero Salado): Buoys No. 20 - 26, 32 - 36 and 39 - 48.
4.- The depths between buoys 39 - 51 recorded by the navigation equipment may vary from the depth on the chart, due to the presence of suspended sediments.
5.- The next aid to navigation, Beacon "Roca Seiba" has Automatic Identification System (AIS).