NOAA ENCŪ

NATIONAL OCEANIC AND ATMOSPHERIC ADMINISTRATION

US4AK7KG - ALASKA


INDEX:

NOTE A
AUTHORITIES
AIDS TO NAVIGATION
WARNING - PRUDENT MARINER
POLLUTION REPORTS
SUPPLEMENTAL INFORMATION
CAUTION - DEPTHS
CAUTION - USE OF RADIO SIGNALS (LIMITATIONS)
COLREGS, 80.1705
WATER LEVELS, CURRENTS, AND TIDES
COMMENTS REQUESTED
ADDITIONAL INFORMATION
RADAR REFLECTORS
CAUTION - QUALITY OF BATHYMETRIC DATA
CAUTION - TEMPORARY CHANGES


NOTES:

NOTE A 
Navigation regulations are published in Chapter 2, U.S. Coast Pilot 9.  Additions or revisions to Chapter 2 are published in the Notice to Mariners.  Information concerning the regulations may be obtained at the Office of the Commander, 17th Coast Guard District in Juneau, Alaska, or at the Office of the District Engineer, Corps of Engineers in Anchorage, Alaska.
Refer to charted regulation section numbers. 


AUTHORITIES
Hydrography (From surveys of 1952-53) and topography by the National Ocean Service, Coast Survey, with additional data from the State of Alaska, the Geological Survey, and U.S. Coast Guard.


AIDS TO NAVIGATION
Consult U.S. Coast Guard Light List for supplemental information concerning aids to navigation.


WARNING - PRUDENT MARINER
The prudent mariner will not rely solely on any single aid to navigation, particularly on floating aids. See U.S. Coast Guard Light List and U.S. Coast Pilot for details.


POLLUTION REPORTS
Report all spills of oil and hazardous substances to the National Response Center via 1-800-424-8802 (toll free), or to the nearest U.S. Coast Guard facility if telephone communication is impossible (33 CFR 153).


SUPPLEMENTAL INFORMATION
Consult U.S. Coast Pilot 9 for important supplemental information.


CAUTION - DEPTHS
Depths may vary as much as 1.8 meters (6 feet) due to iceberg groundings.


CAUTION - USE OF RADIO SIGNALS (LIMITATIONS) 
Limitations on the use of radio signals as aids to marine navigation can be found in the U.S. Coast Guard Light Lists and National Geospatial-Intelligence Agency Publication 117. Radio direction-finder bearings to commercial broadcasting stations are subject to error and should be used with caution.


COLREGS, 80.1705
International Regulations for Preventing Collisions at Sea, 1972. The entire area of this chart falls seaward of the COLREGS Demarcation Line.


WATER LEVELS, CURRENTS, AND TIDES
Real-time water levels, tide predictions, and tidal current predictions are available on the internet from NOAA's Center for Operational Oceanographic Products and Services (CO-OPS) at https://tidesandcurrents.noaa.gov/water_level_info.html and https://tidesandcurrents.noaa.gov/currents_info.html.


COMMENTS REQUESTED
NOAA encourages users to submit inquiries, discrepancies, or comments about this chart via NOAA's ASSIST tool at https://www.nauticalcharts.noaa.gov/customer-service/assist/.


ADDITIONAL INFORMATION
Additional information can be obtained at www.nauticalcharts.noaa.gov.


RADAR REFLECTORS 
Radar reflectors have been placed on many floating aids to navigation. Individual radar reflector identification on these aids has been omitted from this chart.


CAUTION - QUALITY OF BATHYMETRIC DATA
The areas represented by the object M_QUAL (Quality of data) are approximate due to generalizing for clarity. Caution is advised, particularly for nearshore navigation or voyage planning. M_QUAL represents areas of uniform quality of bathymetric data. The CATZOC (Category of zone of confidence in data) attribute of M_QUAL provides an assessment of the overall zone of confidence.


CAUTION - TEMPORARY CHANGES
Temporary changes or defects in aids to navigation are not indicated. See Local Notice to Mariners.


END OF FILE