THE NAVIGABLE CHANNEL:

1.North Approach Channel (Port Said):                         	

1.1. Port Said East Approach Channel from Hm 230 to Hm 0.00 E:

a)From outer pair of light buoys at Hm 230 to Hm 94.90  where it joins the west approach channel.
b)From Hm 94.90 to buoys at Hm 0.00 E.
c)The light beacons at Km 2.738 E.

1.2. Port Said West Approach Channel through Port Said West Port:

a)Approach Channel from Hm 94.90 to buoys at Hm 21.50.
b)Port Said West Port from Hm 21.50 to Km 3.700 (Raswa St.).
c)Port Said old Lighthouse at Hm 0.00.
d)Distance from Fairway buoys to Port Said Lighthouse is 11.040 Km (Bearing 017 degree).

2.Main Channel:

2.1.Double Channel from Hm 0.00 E to Km 17.00:
   2.1.1 West Channel 
        - Port Said Branch from Hm 21.50 to Km 17.000. 
   2.1.2 East Channel 
        - From buoys at Hm 0.00 E to Km 15.450 E.
 
2.2.Single Channel from Km 17.000 to Km 51.660

2.3.Double Channel from Km 51.660 to Km 122.100
   2.3.1 West Channel 
        - from Km 51.660 to Km 122.100
   2.3.2 East Channel 
        - from Km 51.660 to Km 99.302 E (Km 101.942 )
        - from Km 101.942 to Km 122.100 
2.4.Single Channel from Km 122.100 to Km 162.250
