NOAA ENCŪ

NATIONAL OCEANIC AND ATMOSPHERIC ADMINISTRATION

US4AK7ML - ALASKA


INDEX:

NOTE A
AIDS TO NAVIGATION
POLLUTION REPORTS
SUPPLEMENTAL INFORMATION
WARNING - PRUDENT MARINER
COLREGS, 80.1705
AUTHORITIES
CAUTION - MARINERS
CAUTION - DEPTHS
CAUTION - TEMPORARY CHANGES
NOAA WEATHER RADIO BROADCASTS
SUBSISTENCE WHALING IN THE BEAUFORT SEA
WATER LEVELS, CURRENTS, AND TIDES
COMMENTS REQUESTED
RADAR REFLECTORS 
ADMINISTRATION AREA
ADDITIONAL INFORMATION
CAUTION - QUALITY OF BATHYMETRIC DATA
CAUTION - USE OF RADIO SIGNALS (LIMITATIONS)
HORIZONTAL DATUM


NOTES:

NOTE A
Navigation regulations are published in Chapter 2, U.S. Coast Pilot 9.  Additions or revisions to Chapter 2 are published in the Notice to Mariners. Information concerning the regulations may be obtained at the Office of the Commander, 17th Coast Guard District in Juneau, Alaska, or at the Office of the District Engineer, Corps of Engineers in Anchorage, Alaska.
Refer to charted regulation section numbers.


AIDS TO NAVIGATION
Consult U.S. Coast Guard Light List for supplemental information concerning aids to navigation.


POLLUTION REPORTS
Report all spills of oil and hazardous substances to the National Response Center via 1-800-424-8802 (toll free), or to the nearest U.S. Coast Guard facility if telephone communication is impossible (33 CFR 153).


SUPPLEMENTAL INFORMATION
Consult U.S. Coast Pilot 9 for important supplemental information.


WARNING - PRUDENT MARINER
The prudent mariner will not rely solely on any single aid to navigation, particularly on floating aids. See U.S. Coast Guard Light List and U.S. Coast Pilot for details.


COLREGS, 80.1705
International Regulations for Preventing Collisions at Sea, 1972. The entire area of this chart falls seaward of the COLREGS Demarcation Line.


AUTHORITIES
Hydrography and topography by the National Ocean Service, Coast Survey, with additional data from the State of Alaska, Geological Survey and U.S. Coast Guard.


CAUTION - MARINERS
Mariners are advised that in the shallow waters of the Beaufort Sea, water levels are strongly influenced by meteorological conditions. Strong offshore winds can produce water depths up to 0.8 meters (2.6 feet) less than those shown.


CAUTION - DEPTHS
Depths may vary as much as 1.8 meters (6 feet) due to iceberg groundings.


CAUTION - TEMPORARY CHANGES
Temporary changes or defects in aids to navigation are not indicated.  See Local Notice to Mariners


NOAA WEATHER RADIO BROADCASTS
The NOAA Weather Radio station listed below provides continuous weather broadcasts. The reception range is typically 20 to 40 nautical miles from the antenna site, but can be as much as 100 nautical miles for stations at high elevations.

Barrow, AK	KZZ-53		162.550 MHz


SUBSISTENCE WHALING IN THE BEAUFORT SEA
Mariners should be aware that Alaskan Natives engage in subsistence whaling in the Beaufort Sea from August 15 to October 31. Vessel operators are requested to contact the Alaska Eskimo Whaling Commission at (907) 852-2392, or aewcdir@barrow.com prior to entering this area for information about the location and avoidance of traditional Native hunting parties.


WATER LEVELS, CURRENTS, AND TIDES
Real-time water levels, tide predictions, and tidal current predictions are available on the internet from NOAA's Center for Operational Oceanographic Products and Services (CO-OPS) at https://tidesandcurrents.noaa.gov/water_level_info.html and https://tidesandcurrents.noaa.gov/currents_info.html.


COMMENTS REQUESTED
NOAA encourages users to submit inquiries, discrepancies, or comments about this chart via NOAA's ASSIST tool at https://www.nauticalcharts.noaa.gov/customer-service/assist/.


RADAR REFLECTORS 
Radar reflectors have been placed on many floating aids to navigation. Individual radar reflector identification on these aids has been omitted from this chart.


ADMINISTRATION AREA
The entire extent of this ENC cell falls within the limits of an Administration Area. This area covers land, internal waters, and territorial sea.  The territorial sea is a maritime zone which the United States exercises sovereignty extending to the airspace as well as to its bed and subsoil.  For more information, please refer to the Coast Pilot.


ADDITIONAL INFORMATION
Additional information can be obtained at www.nauticalcharts.noaa.gov.


CAUTION - QUALITY OF BATHYMETRIC DATA
The areas represented by the object M_QUAL (Quality of data) are approximate due to generalizing for clarity. Caution is advised, particularly for nearshore navigation or voyage planning. M_QUAL represents areas of uniform quality of bathymetric data. The CATZOC (Category of zone of confidence in data) attribute of M_QUAL provides an assessment of the overall zone of confidence.


CAUTION - USE OF RADIO SIGNALS (LIMITATIONS)
Limitations on the use of radio signals as aids to marine navigation can be found in the U.S. Coast Guard Light Lists and National Geospatial-Intelligence Agency Publication 117. Radio direction-finder bearings to commercial broadcasting stations are subject to error and should be used with caution.


HORIZONTAL DATUM 
The NOAA ENC references the World Geodetic System of 1984 (WGS-84). For charting purposes, the horizontal control of the current realization of WGS-84 is functionally equivalent to the International Terrestrial Reference Frame 2020 (ITRF2020) at the meter level for charts at scales of 1:5,000 or smaller.


END OF FILE